|  |  |  |  |
| --- | --- | --- | --- |
| Item | Assumptions | Value | Sources |
| Electric Boards | * The functional unit has been defined as the Electric Induction **Left** Printed Circuit Board assembly (ELINRPCBA), Electric Induction **Right** Printed Circuit Board Assembly (ELINLPCBA) and Touch Control Printed Circuit Board Assembly (TCPCBA) used in a cooktop with 4 induction hobs. * This induction ceramic hob has a width of 60 cm, and 7200 W of power at a voltage of 220e240 V and a frequency between 50 and 60 Hz. * 4 cooking zones, each one with variable 17-stage power settings. * Made and used in Spain * Weight: 0.8168246kg * Cradle to Gate | 71.82kg CO2-eq/unit | [Link](https://drive.google.com/file/d/0B--O_p54KxzvVUVxRXlQR2VwZjQ/view?usp=sharing) |
| Ceramic Glass | * 583mm x 513mm x 5mm * Assumed toughened glass (conventional): 1.35 CO2-eq/kg * Thickness assumed at 5mm * 2.5lb/ft^2 * Area: 299,079mm^2 * Weight=1.46kg | 1.97kg CO2-eq/unit | [Link](http://www.us.schott.com/pyran/english/products/pyran_platinumf.html) |
| BOSCH 60cm Induction Ceramic Hob *-minus-* Electrical *-minus-* Glass | * 55mm x 583mm x 513 mm * Weight before subtraction (kg):11.0 kg * Assumed Stainless Steel: 6.15 kg CO2/kg (CO2only) * Weight after subtraction: 8.7231754kg | 53.65kg CO2-eq/unit | [Link1](http://www.bosch-home.com.sg/store/product/PIE645F17E/PIE645F17E#tab5) |
| Total |  | 127.44 kg CO2-eq/unit |  |