|  |  |  |
| --- | --- | --- |
| PV Type | kg CO2 / m^2 | Link |
| Monocrystalline (avg) | 242 | [Link](http://www.greenspec.co.uk/building-design/embodied-energy/) |
| Polycrystalline (avg) | 208 |
| Thin Film | 67 |