|  |  |  |  |
| --- | --- | --- | --- |
| **Item** | **Assumptions** | **Value** | **Source** |
| Conventional | * LCA data centered in Japan * Toilet bowl replaced every 13 years; showerhead every 20 * No model or brand given for either plumbing fixture: assumed generic | 100.5 kg CO2-eq | [Link](https://drive.google.com/file/d/0B--O_p54KxzvWEl5ZkxMSFoxMUU/view?usp=sharing) |